# Bathymetry Hillshade [2m]--Offshore of Monterey, California

### Metadata:

- Identification_Information
- Data_Quality_Information
- Spatial_Data_Organization_Information
- Spatial_Reference_Information
- Entity_and_Attribute_Information
- Distribution_Information
- Metadata_Reference_Information

Identification_Information:
Citation:
Citation_Information:
Originator: Peter Dartnell
Originator: Rikk G. Kvitek
Publication_Date: 2016
Title: Bathymetry Hillshade [2m]--Offshore of Monterey, California
Edition: 1.0
Geospatial_Data_Presentation_Form: GeoTiff
Series_Information:
Series_Name: Data Series
Issue_Identification: DS 781
Publication_Information:
Publication_Place: Reston, VA
Publisher: U.S. Geological Survey
Online_Linkage: https://doi.org/10.3133/ds781
Online_Linkage:
https://cmgds.marine.usgs.gov/data/csmp/OffshoreMonterey/data_catalog_OffshoreMonterey.html
Larger_Work_Citation:
Citation_Information:
Originator: Nadine E. Golden
Publication_Date: 2015
Title: California State Waters Map Series Data Catalog
Geospatial_Data_Presentation_Form: database
Series_Information:
Series_Name: Data Series
Issue_Identification: DS 781
Publication_Information:
Publication_Place: Reston, VA
Publisher: U.S. Geological Survey
Online_Linkage: https://doi.org/10.3133/ds781
Description:
Abstract:
This part of DS 781 presents data for the bathymetry map of the Offshore of Monterey map area, California. Bathymetry data are provided as separate grids depending on resolution. This metadata file refers to the data included in "BathymetryHS_2m_OffshoreMonterey.zip," which is accessible from https://doi.org/10.5066/F70Z71C8. These data accompany the pamphlet and map sheets of Johnson, S.Y., Dartnell, P., Hartwell, S.R., Cochrane, G.R., Golden, N.E., Watt, J.T., Davenport, C.W., Kvitek, R.G., Erdey, M.D., Krigsman, L.M., Sliter, R.W., and Maier, K.L. (S.Y. Johnson and S.A. Cochran, eds.), 2016, California State Waters Map Series—Offshore of Monterey, California: U.S. Geological Survey Open-File Report 2016–1110, pamphlet 44 p., 10 sheets, scale 1:24,000, https://doi.org/10.3133/ofr20161110.
The 2-m and 5-m bathymetry and shaded-relief bathymetry maps of the Offshore of Monterey map area, California, were generated from acoustic bathymetry data collected by California State University, Monterey Bay (CSUMB) and by Monterey Bay Aquarium Research Institute (MBARI), as well as from bathymetric lidar data collected by the U.S. Army Corps of Engineers, Joint Airborne Lidar Bathymetry Center of Expertise (JALBTCX). Acoustic mapping was completed between 1998 and 2012 using a combination of 200-kHz/400-kHz Reson 7125, 100-kHz Reson 7111, 240-kHz Reson 8101, and 30-kHz Simrad EM-300 multibeam echosounders, as well as 234-kHz and 468-kHz SWATHplus bathymetric sidescan-sonar systems. Bathymetric lidar mapping was completed between 2009 and 2010 for the California Coastal Mapping Project (CCMP). These mapping missions combined to collect bathymetry data from the shoreline to beyond the limit of California’s State Waters. NOTE: The horizontal datum of this bathymetry data (NAD83) differs from the horizontal datum of other layers in this data release (WGS84).
Purpose:
These data are intended for science researchers, students, policy makers, and the general public. These data can be used with geographic information systems or other software to identify bathymetric features. These data are not intended to be used for navigation.
Supplemental_Information:
For additional information CSUMB on bathymetry data online visit http://seafloor.otterlabs.org and for MBARI data see http://www.ngdc.noaa.gov/mgg/bathymetry/relief.html.
Time_Period_of_Content:
Time_Period_Information:
Range_of_Dates/Times:
Beginning_Date: 1998
Ending_Date: 2012
Currentness_Reference: ground condition
Status:
Progress: Complete
Maintenance_and_Update_Frequency: As needed
Spatial_Domain:
Bounding_Coordinates:
West_Bounding_Coordinate: -122.064886
East_Bounding_Coordinate: -121.811775
North_Bounding_Coordinate: 36.692799
South_Bounding_Coordinate: 36.532722
Keywords:
Theme:
Theme_Keyword_Thesaurus: USGS Metadata Identifier
Theme_Keyword: USGS:8de1c4e2-e028-4045-95bc-2b5c2e0b95b6
Theme:
Theme_Keyword_Thesaurus: Global Change Master Directory (GCMD)
Theme_Keyword: Bathymetry
Theme_Keyword: Seafloor Topography
Theme:
Theme_Keyword_Thesaurus: None
Theme_Keyword: Seafloor Character
Theme_Keyword: Fisheries
Theme_Keyword: Ecosystem
Theme_Keyword: Multibeam
Theme_Keyword: Geology
Theme_Keyword: Bathymetry
Theme_Keyword: Backscatter
Theme_Keyword: Intensity
Theme_Keyword: Ocean Floor Topography
Theme_Keyword: U.S. Geological Survey
Theme_Keyword: USGS
Theme_Keyword: Coastal and Marine Hazards and Resources Program
Theme_Keyword: CMHRP
Theme_Keyword: Pacific Coastal and Marine Science Center
Theme_Keyword: PCMSC
Theme:
Theme_Keyword_Thesaurus: ISO 19115 Topic Category
Theme_Keyword: geoscientificInformation
Theme_Keyword: environment
Theme_Keyword: oceans
Theme_Keyword: imageryBaseMapsEarthCover
Theme:
Theme_Keyword_Thesaurus: Data Categories for Marine Planning
Theme_Keyword: distributions
Theme_Keyword: bathymetry and elevation
Theme:
Theme_Keyword_Thesaurus: USGS Thesaurus
Theme_Keyword: sonar methods
Theme_Keyword: bathymetry measurement
Theme_Keyword: bathymetry
Theme_Keyword: marine geophysics
Theme:
Theme_Keyword_Thesaurus: Coastal and Marine Ecological Classification Standard (CMECS)
Theme_Keyword: Marine Nearshore Subtidal
Theme_Keyword: Marine Offshore Subtidal
Theme_Keyword: Transform Continental Margin
Theme_Keyword: Continental/Island Shelf
Theme_Keyword: Rock Substrate
Theme_Keyword: Unconsolidated Mineral Substrate
Place:
Place_Keyword_Thesaurus: Geographic Names Information System (GNIS)
Place_Keyword: Pacific Ocean
Place_Keyword: State of California
Place_Keyword: Monterey
Place_Keyword: Monterey County
Place_Keyword: Seaside
Place_Keyword: Marina
Place:
Place_Keyword_Thesaurus: Coastal and Marine Ecological Classification Standard (CMECS)
Place_Keyword: Northern California Ecoregion
Stratum:
Stratum_Keyword_Thesaurus: Coastal and Marine Ecological Classification Standard (CMECS)
Stratum_Keyword: Substrate
Access_Constraints: None
Use_Constraints:
USGS-authored or produced data and information are in the public domain. Acknowledge the U.S. Geological Survey and California State University, Monterey Bay, Seafloor Mapping Lab in products derived from these data. Share data products developed using these data with the U.S. Geological Survey. This information is not intended for navigational purposes. Read and fully comprehend the metadata prior to data use. Uses of these data should not violate the spatial resolution of the data. Where these data are used in combination with other data of different resolution, the resolution of the combined output will be limited by the lowest resolution of all the data. This database has been approved for release and publication by the Director of the USGS. Although this database has been subjected to rigorous review and is substantially complete, the USGS reserves the right to revise the data pursuant to further analysis and review. Furthermore, it is released on condition that neither the USGS nor the United States Government may be held liable for any damages resulting from its authorized or unauthorized use. Although this Federal Geographic Data Committee-compliant metadata file is intended to document these data in nonproprietary form, as well as in ArcInfo format, this metadata file may include some ArcInfo-specific terminology.
Point_of_Contact:
Contact_Information:
Contact_Organization_Primary:
Contact_Organization:
U.S. Geological Survey, Pacific Coastal and Marine Science Center
Contact_Person: PCMSC Science Data Coordinator
Contact_Address:
Address_Type: mailing and physical
Address: 2885 Mission Street
City: Santa Cruz
State_or_Province: CA
Postal_Code: 95060-5792
Country: US
Contact_Voice_Telephone: 831-427-4747
Contact_Electronic_Mail_Address: pcmsc_data@usgs.gov
Browse_Graphic:
Browse_Graphic_File_Name:
https://www.sciencebase.gov/catalog/file/get/56cf5fc5e4b015c306ed183c?name=BathymetryHS_2m_OffshoreMonterey.jpg&allowOpen=true
Browse_Graphic_File_Description: Hillshaded bathymetry map offshore of Monterey.
Browse_Graphic_File_Type: JPEG
Native_Data_Set_Environment:
Microsoft Windows Server 2008 R2 Version 6.1 (Build 7601) Service Pack 1; ESRI ArcCatalog 10.0
Cross_Reference:
Citation_Information:
Originator: Johnson, S.Y.
Originator: Dartnell, P.
Originator: Hartwell, S.R.
Originator: Cochrane, G.R.
Originator: Golden, N.E.
Originator: Watt, J.T.
Originator: Davenport, C.W.
Originator: Kvitek, R.G.
Originator: Erdey, M.D.
Originator: Krisgman, L.M.
Originator: Sliter, R.W.
Originator: Maier, K.L.
Publication_Date: 2016
Title:
California State Waters Map Series--Offshore of Monterey, California
Series_Information:
Series_Name: Open-File Report
Issue_Identification: 2016-1110
Publication_Information:
Publication_Place: Reston, VA
Publisher: U.S. Geological Survey
Online_Linkage: https://doi.org/10.3133/ofr20161110
Data_Quality_Information:
Attribute_Accuracy:
Attribute_Accuracy_Report: Not applicable for raster data.
Logical_Consistency_Report: Unspecified
Completeness_Report: Complete
Positional_Accuracy:
Horizontal_Positional_Accuracy:
Horizontal_Positional_Accuracy_Report:
Estimated to be no less than 2 m, owing to water depth and total propagated uncertainties of the mapping systems, which include sonar system, position and motion compensation system, and navigation, as well as data processing that includes sounding cleaning, gridding, and datum transformations.
Vertical_Positional_Accuracy:
Vertical_Positional_Accuracy_Report:
Estimated to be no less than 20 cm, owing to water depth and total propagated uncertainties of the mapping systems, which include sonar system, position and motion compensation system, and navigation, as well as data processing that includes sounding cleaning, gridding, and datum transformations.
Lineage:
Process_Step:
Process_Description:
During the CSUMB mapping missions, an Applanix POS MV (Position and Orientation System for Marine Vessels) was used to accurately position the vessels during data collection, and it also accounted for vessel motion such as heave, pitch, and roll (position accuracy, +/-2 m; pitch, roll, and heading accuracy, +/-0.02 percent; heave accuracy, +/-5 percent, or 5 cm). To account for tidal-cycle fluctuations, KGPS data (GPS data with real-time kinematic corrections) was used; in addition, sound-velocity profiles were collected with an Applied Microsystems (AM) SVPlus sound velocimeter. Soundings were corrected for vessel motion using the Applanix POS MV data, for variations in water-column sound velocity using the AM SVPlus data, and for variations in water height (tides) using vertical-position data from the KGPS receivers. Finally, the soundings were converted into 2-m-resolution bathymetric-surface-model grids.
Process_Date: 2006
Process_Contact:
Contact_Information:
Contact_Person_Primary:
Contact_Person: Carrie Bretz
Contact_Organization: Seafloor Mapping Lab, California State University Monterey Bay
Contact_Position: Projects Manager, GIS & Metadata Supervisor
Contact_Address:
Address_Type: mailing and physical address
Address: 100 Campus Center, Bldg 13
City: Seaside
State_or_Province: CA
Postal_Code: 93955
Country: USA
Contact_Voice_Telephone: 831.582.4197
Contact_Electronic_Mail_Address: carrie_bretz@csumb.edu
Process_Step:
Process_Description:
Nearshore acoustic and lidar bathymetric data within California State Waters were merged together by Dewberry as part of the 2013 NOAA Coastal California TopoBathy Merge Project (National Oceanic and Atmospheric Administration, 2013). Merged bathymetry data within the Southern Monterey Bay map area were downloaded from this data set and re-sampled to 2-m spatial resolution. The MBARI 5-m bathymetric surface-model-grid was also clipped to the Offshore of Monterey map boundary. The 2-m and 5-m grids were not merged and are provided as separate grids. To create the shaded-relief imagery, an illumination having an azimuth of 300 degrees and 45 degrees above the horizon was applied to the bathymetry grids.
Process_Date: 2016
Process_Contact:
Contact_Information:
Contact_Person_Primary:
Contact_Person: Pete Dartnell
Contact_Organization:
U.S. Geological Survey, Pacific Coastal and Marine Science Center
Contact_Position: Physical Scientist
Contact_Address:
Address_Type: mailing and physical address
Address: 2885 Mission St.
City: Santa Cruz
State_or_Province: CA
Postal_Code: 95060-5792
Country: USA
Contact_Voice_Telephone: (831) 460-7415
Contact_Electronic_Mail_Address: pdartnell@usgs.gov
Process_Step:
Process_Description:
Keywords section of metadata optimized for discovery in USGS Coastal and Marine Geology Data Catalog.
Process_Date: 20171005
Process_Contact:
Contact_Information:
Contact_Organization_Primary:
Contact_Organization: U.S. Geological Survey
Contact_Person: Alan O. Allwardt
Contact_Position: Contractor -- Information Specialist
Contact_Address:
Address_Type: mailing and physical address
Address: 2885 Mission Street
City: Santa Cruz
State_or_Province: CA
Postal_Code: 95060
Contact_Voice_Telephone: 831-460-7551
Contact_Facsimile_Telephone: 831-427-4748
Contact_Electronic_Mail_Address: aallwardt@usgs.gov
Process_Step:
Process_Description:
Added keywords from Coastal and Marine Ecological Classification Standard (CMECS) to metadata.
Process_Date: 20180426
Process_Contact:
Contact_Information:
Contact_Organization_Primary:
Contact_Organization: U.S. Geological Survey
Contact_Person: Alan O. Allwardt
Contact_Position: Contractor -- Information Specialist
Contact_Address:
Address_Type: mailing and physical address
Address: 2885 Mission Street
City: Santa Cruz
State_or_Province: CA
Postal_Code: 95060
Contact_Voice_Telephone: 831-460-7551
Contact_Facsimile_Telephone: 831-427-4748
Contact_Electronic_Mail_Address: aallwardt@usgs.gov
Process_Step:
Process_Description:
Edited metadata to add keywords section with USGS persistent identifier as theme keyword. No data were changed.
Process_Date: 20201019
Process_Contact:
Contact_Information:
Contact_Organization_Primary:
Contact_Organization: U.S. Geological Survey
Contact_Person: VeeAnn A. Cross
Contact_Position: Marine Geologist
Contact_Address:
Address_Type: Mailing and Physical
Address: 384 Woods Hole Road
City: Woods Hole
State_or_Province: MA
Postal_Code: 02543-1598
Contact_Voice_Telephone: 508-548-8700 x2251
Contact_Facsimile_Telephone: 508-457-2310
Contact_Electronic_Mail_Address: vatnipp@usgs.gov
Process_Step:
Process_Description:
Performed minor edits to the metadata to correct typos. No data were changed
Process_Date: 20211014
Process_Contact:
Contact_Information:
Contact_Organization_Primary:
Contact_Organization: U.S. Geological Survey
Contact_Person: Susan A. Cochran
Contact_Position: Geologist
Contact_Address:
Address_Type: Mailing and Physical
Address: 2885 Mission Street
City: Santa Cruz
State_or_Province: CA
Postal_Code: 95060
Contact_Voice_Telephone: 831-460-7545
Contact_Electronic_Mail_Address: scochran@usgs.gov
Process_Step:
Process_Description:
Edits were made to bring the metadata up to current PCMSC standards including standardizing authors' names, adding a doi# link, correcting typos, refining keywords, and using current access and distribution liability statements. Point of Contact and Metadata Contact information sections were changed to static PCMSC contact information. No data were changed. The metadata available from a harvester may supersede metadata bundled within a download file. Users are advised to compare the metadata date of this file to any similar file to ensure they are using the most recent version.
Process_Date: 20220520
Process_Contact:
Contact_Information:
Contact_Organization_Primary:
Contact_Organization: U.S. Geological Survey
Contact_Person: Susan A. Cochran
Contact_Position: Geologist
Contact_Address:
Address_Type: Mailing and Physical
Address: 2885 Mission Street
City: Santa Cruz
State_or_Province: CA
Postal_Code: 95060
Contact_Voice_Telephone: 831-460-7545
Contact_Electronic_Mail_Address: scochran@usgs.gov
Spatial_Data_Organization_Information:
Direct_Spatial_Reference_Method: Raster
Raster_Object_Information:
Raster_Object_Type: Grid Cell
Row_Count: 11222
Column_Count: 8816
Vertical_Count: 1
Spatial_Reference_Information:
Horizontal_Coordinate_System_Definition:
Planar:
Grid_Coordinate_System:
Grid_Coordinate_System_Name: Universal Transverse Mercator
Universal_Transverse_Mercator:
UTM_Zone_Number: 10
Transverse_Mercator:
Scale_Factor_at_Central_Meridian: 0.9996
Longitude_of_Central_Meridian: -123.00000
Latitude_of_Projection_Origin: 0.00000
False_Easting: 500000.0
False_Northing: 0.00
Planar_Coordinate_Information:
Planar_Coordinate_Encoding_Method: coordinate pair
Coordinate_Representation:
Abscissa_Resolution: 2.0
Ordinate_Resolution: 2.0
Planar_Distance_Units: Meters
Geodetic_Model:
Horizontal_Datum_Name: NAD83
Ellipsoid_Name: GRS80
Semi-major_Axis: 6378137.00
Denominator_of_Flattening_Ratio: 298.257223563
Vertical_Coordinate_System_Definition:
Altitude_System_Definition:
Altitude_Datum_Name: North American Vertical Datum of 1988
Altitude_Resolution: 2.0
Altitude_Distance_Units: meters
Altitude_Encoding_Method: Attribute values
Entity_and_Attribute_Information:
Detailed_Description:
Entity_Type:
Entity_Type_Label: Value
Entity_Type_Definition: Bathymetry [2m] hillshade intensity value
Entity_Type_Definition_Source: ESRI
Attribute:
Attribute_Label: VALUE
Attribute_Definition: Bathymetry hillshade intensity value
Attribute_Definition_Source: ESRI
Attribute_Domain_Values:
Range_Domain:
Range_Domain_Minimum: 0
Range_Domain_Maximum: 254
Attribute_Units_of_Measure: Integers from 0-254 representing hillshaded bathymetry
Overview_Description:
Entity_and_Attribute_Overview:
The complete 2-m resolution bathymetry grid for Offshore of Monterey, California were originally archived as an ESRI grid with the following attributes. NOTE: the horizontal datum of the bathymetry data (NAD83) differs from the horizontal datum of other layers in this data release (WGS84).

    Cell size = 2.0
    Number of rows = 11222
    Number of columns = 8816

    Data type = floating point

    Boundary
    Xmin = 583710
    Xmax = 606154
    Ymin = 4043571
    Ymax = 4061203

    Statistics
    Minimum value = 0
    Maximum value = 254
    Mean = 179.95
    Standard deviation = 23.80

    Coordinate system description
    Projection  UTM
    Zone  10
    Datum  NAD83
    Vertical Datum  NAVD88
    Units  meter

Entity_and_Attribute_Detail_Citation: none
Distribution_Information:
Distributor:
Contact_Information:
Contact_Organization_Primary:
Contact_Organization: U.S. Geological Survey
Contact_Address:
Address_Type: mailing and physical address
Address: 345 Middlefield Rd
City: Menlo Park
State_or_Province: CA
Postal_Code: 94025-3561
Country: USA
Contact_Voice_Telephone: (650) 329-4309
Distribution_Liability:
These databases, identified as bathymetry and shaded-relief maps of the Offshore of Monterey map area, California have been approved for release and publication by the U.S. Geological Survey (USGS). Although these databases have been subjected to rigorous review and are substantially complete, the USGS reserves the right to revise the data pursuant to further analysis and review. Furthermore, it is released on condition that neither the USGS nor the United States Government may be held liable for any damages resulting from its authorized or unauthorized use. Although these data have been processed successfully on a computer system at the U.S. Geological Survey (USGS), no warranty expressed or implied is made regarding the display or utility of the data on any other system or for general or scientific purposes, nor shall the act of distribution constitute any such warranty. The USGS or the U.S. Government shall not be held liable for improper or incorrect use of the data described and/or contained herein. Reference herein to any specific commercial product, process, or service by trade name, trademark, manufacturer, or otherwise does not constitute or imply its endorsement, recommendation, or favoring by the United States Government or any agency thereof. These data are not intended for navigational use.
Standard_Order_Process:
Digital_Form:
Digital_Transfer_Information:
Format_Name: TIFF
Format_Version_Number: ArcMap (version 10.0, ESRI , 2011)
Format_Specification:
Raster data layer is registered TIFF image in the UTM Zone 10 coordinate system with datum NAD83.
Format_Information_Content:
The .zip file for the TIFF image includes the image (.tif), the world registration file (.tfw), and FGDC-compliant metadata for the BathymetryA [2m] data layer of Offshore Monterey, California.
File_Decompression_Technique: WinZip
Transfer_Size: 38
Digital_Transfer_Option:
Online_Option:
Computer_Contact_Information:
Network_Address:
Network_Resource_Name:
https://www.sciencebase.gov/catalog/file/get/56d61a72e4b015c306f27054?
Network_Resource_Name: https://doi.org/10.5066/F70Z71C8
Network_Resource_Name: https://pubs.usgs.gov/ds/781/
Access_Instructions:
Data can be downloaded using the Network Resource links. The first link will begin a direct download of the data. The second link is a landing page on which all of the downloadable data for a particular region are listed. The third link is a landing page for the entire data catalog.
Fees: none
Technical_Prerequisites:
The downloadable data file has been compressed with the "zip" command and can be unzipped with Winzip (or other tool) on Windows systems. To utilize these data, the user must have software capable of uncompressing the WinZip file and importing and viewing an Esri ArcMap TIFF. Users should download the ArcGIS Project File, OffshoreMontereyGIS.mxd.zip, a compressed (with the "zip" command) version of the ArcMap document (.mxd) that has all the data layers loaded in the table of contents for "Offshore of Monterey map area" and has all the data symbolized as on the data release map sheets. Download and save this ArcGIS project file, including all data layers, to the directory the user has created for this GIS.
Metadata_Reference_Information:
Metadata_Date: 20220520
Metadata_Contact:
Contact_Information:
Contact_Organization_Primary:
Contact_Organization:
U.S. Geological Survey, Pacific Coastal and Marine Science Center
Contact_Person: PCMSC Science Data Coordinator
Contact_Address:
Address_Type: mailing and physical
Address: 2885 Mission Street
City: Santa Cruz
State_or_Province: CA
Postal_Code: 95060-5792
Country: US
Contact_Voice_Telephone: 831-427-4747
Contact_Electronic_Mail_Address: pcmsc_data@usgs.gov
Metadata_Standard_Name: Content Standard for Digital Geospatial Metadata
Metadata_Standard_Version: FGDC-STD-001-1998
Metadata_Time_Convention: local time

Generated by mp version 2.9.52 on Fri May 20 14:58:20 2022