# H11250G_HS: 2-m Hill-Shaded Bathymetric Grid of NOAA Survey H11250 of The Race (Geographic)

Metadata also available as Outline | Text

## Metadata:

- Identification_Information
- Data_Quality_Information
- Spatial_Data_Organization_Information
- Spatial_Reference_Information
- Entity_and_Attribute_Information
- Distribution_Information
- Metadata_Reference_Information

Identification_Information:
  Citation:
    Citation_Information:
      Originator: U.S. Geological Survey
      Publication_Date: 2007
      Title:
        H11250G_HS: 2-m Hill-Shaded Bathymetric Grid of NOAA Survey H11250 of The Race (Geographic)
      Edition: 1.0
      Geospatial_Data_Presentation_Form: raster digital data
      Series_Information:
        Series_Name: Open-File Report
        Issue_Identification: 2007-1012
      Publication_Information:
        Publication_Place: Woods Hole Science Center, Woods Hole, MA
        Publisher: U.S. Geological Survey, Coastal and Marine Geology Program
      Online_Linkage:
        <http://pubs.usgs.gov/of/2007/1012/data/bathy/grids/geo/h11250_geo_hlshd2m/h11250g_hs.zip>
      Online_Linkage: <http://pubs.usgs.gov/of/2007/1012/html/catalog.html>
      Larger_Work_Citation:
        Citation_Information:
          Originator: L.J. Poppe
          Originator: M.L. DiGiacomo-Cohen
          Originator: E.F. Doran
          Originator: S.M. Smith
          Originator: H.F. Stewart
          Originator: N.A. Forfinski
          Publication_Date: 2007
          Title:
            Geologic Interpretation and Multibeam Bathymetry of the Sea Floor in the Vicinity of the Race, Eastern Long Island Sound
          Edition: 1.0
          Series_Information:
            Series_Name: Open-File Report
            Issue_Identification: 2007-1012
          Publication_Information:
            Publication_Place: Woods Hole Science Center, Woods Hole, MA
            Publisher: Coastal and Marine Geology Program, U.S. Geological Survey
          Other_Citation_Details: Also available on DVD-ROM
          Online_Linkage: <http://pubs.usgs.gov/of/2007/1012/>
  Description:
    Abstract:
      The U.S. Geological Survey, in cooperation with the National Oceanic and Atmospheric Administration and the Connecticut Department of Environmental Protection, has produced detailed geologic maps of the sea floor in Long Island Sound, a major East Coast estuary surrounded by the most densely populated region of the United States. These studies have built upon cooperative research with the State of Connecticut that was initiated in 1982. The current phase of this research program is directed toward studies of sea-floor sediment distribution, processes that control sediment distribution, nearshore environmental concerns, and the relation of benthic community structures to the sea-floor geology.

      Anthropogenic wastes, toxic chemicals, and changes in land-use patterns resulting from residential, commercial, and recreational development have stressed the environment of the Sound, causing degradation and potential loss of benthic habitats (Koppelman and others, 1976; Long Island Sound Study, 1994). Detailed maps of the sea floor are needed to help evaluate the extent of adverse impacts and to help manage resources wisely in the future. Therefore, in a continuing effort to better understand Long Island Sound, we have constructed and interpreted mulitbeam bathymetric data within specific areas of special interest. The gridded data presented herein covers a roughly 94 km square area of the sea floor in the area known as the Race at the eastern end of Long Island Sound. The original multibeam bathymetric data were collected during October 2003 as part of charting applications aboard the NOAA Survey Vessel Thomas Jefferson. A Simrad EM1002 multibeam system mounted on the hull of this vessel was used to acquire over 560 km of survey lines from the deeper water (>20 m) parts of the study area. Two 29-foot launches with hull-mounted Reson systems were deployed from the ship and were used to acquire an additional 637 km of survey lines from the shallower areas.

      The detailed bathymetic data and their interpretations serve many purposes, including: (1) defining the geological variability of the sea floor, which is one of the primary controls of benthic habitat diversity; (2) improving our understanding of the processes that control the distribution and transport of bottom sediments and the distribution of benthic habitats and associated infaunal community structures; and (3) providing a detailed framework for future research, monitoring, and management activities. The bathymetric data models also serve as base maps for subsequent sedimentological, geochemical, and biological observations, because precise information on environmental setting is important for selection of sampling sites and for accurate interpretation of point measurements.

    Purpose:
      The purpose of this datalayer is to release a 2-m hill-shaded grid of NOAA survey H11250 in easternmost Long Island Sound and westernmost Block Island Sound. This GIS layer represents a hillshade of the bathymetric grid H11250G. It was created with the sun at an azimuth of 315, altitude angle above the horizon of 30, and a verticle exaggeration of ~10x. This data set serves a starting point for a geologic study of the area surrounding the Race Long Island Sound. As interpretative layers and images are created they will be added to the GIS database. This gridded data can be used in ArcMap or ArcView to dramatically display the varied bathymetry and geologic features of the area.
  Time_Period_of_Content:
    Time_Period_Information:
      Single_Date/Time:
        Calendar_Date: 2003
    Currentness_Reference: ground condition
  Status:
    Progress: Complete
    Maintenance_and_Update_Frequency: None planned
  Spatial_Domain:
    Bounding_Coordinates:
      West_Bounding_Coordinate: -72.154000
      East_Bounding_Coordinate: -71.992004
      North_Bounding_Coordinate: 41.270996
      South_Bounding_Coordinate: 41.188000
  Keywords:
    Theme:
      Theme_Keyword_Thesaurus: General
      Theme_Keyword: U.S. Geological Survey
      Theme_Keyword: USGS
      Theme_Keyword: National Oceanic and Atmospheric Administration
      Theme_Keyword: NOAA
      Theme_Keyword: Woods Hole Science Center
      Theme_Keyword: NOAA Ship Thomas Jefferson
      Theme_Keyword: grid
      Theme_Keyword: ArcGIS
      Theme_Keyword: multibeam bathymetry
      Theme_Keyword: Long Island Sound Resource Center
      Theme_Keyword: LISRC
      Theme_Keyword: bathymetry
      Theme_Keyword: multibeam bathymetry
      Theme_Keyword: H11250
      Theme_Keyword: NOAA Survey H11250
      Theme_Keyword: hill shaded
      Theme_Keyword: sun illuminated
      Theme_Keyword: Open-File Report 2007-1012
      Theme_Keyword: OFR2007-1012
      Theme_Keyword: NOAA Project Identifier OPR-B370-TJ
      Theme_Keyword: shaded relief
      Theme_Keyword: ArcRaster grid
      Theme_Keyword: WHSC
      Theme_Keyword: Coastal and Marine Geology Program
      Theme_Keyword: CMGP
      Theme_Keyword: Connecticut Department of Envrionmental Protection
      Theme_Keyword: CTDEP
    Theme:
      Theme_Keyword_Thesaurus: ISO 19115 Topic Category
      Theme_Keyword: oceans and estuaries
      Theme_Keyword: oceans and coastal
      Theme_Keyword: elevation
    Place:
      Place_Keyword_Thesaurus: General
      Place_Keyword: North America
      Place_Keyword: United States
      Place_Keyword: Atlantic Ocean
      Place_Keyword: North Atlantic Ocean
      Place_Keyword: northeast United States
      Place_Keyword: Long Island Sound
      Place_Keyword: Connecticut
      Place_Keyword: U.S. East Coast
      Place_Keyword: New York
      Place_Keyword: The Race
      Place_Keyword: Block Island Sound
  Access_Constraints: None
  Use_Constraints:
    Data are not to be used for for navigation purposes.

    Public domain data are freely redistributable with proper metadata and source attribution. Please recognize the U.S. Geological Survey (USGS) and the Connecticut Department of Environmental Protection (CTDEP) as the originators of this dataset.

  Point_of_Contact:
    Contact_Information:
      Contact_Organization_Primary:
        Contact_Organization: U.S. Geological Survey
        Contact_Person: Larry Poppe
      Contact_Position: Geologist
      Contact_Address:
        Address_Type: mailing and physical address
        Address: 384 Woods Hole Road
        City: Woods Hole
        State_or_Province: MA
        Postal_Code: 02543-1598
        Country: USA
      Contact_Voice_Telephone: 508-548-8700 x2314
      Contact_Facsimile_Telephone: 508-457-2310
      Contact_Electronic_Mail_Address: lpoppe@usgs.gov
  Browse_Graphic:
    Browse_Graphic_File_Name:
      <http://pubs.usgs.gov/of/2007/1012/data/bathy/grids/geo/h11250_geo_hlshd2m/h11250g_hs.gif>
    Browse_Graphic_File_Description:
      Thumbnail of the hill-shaded relief map of the H11250 study area created in ArcMap
    Browse_Graphic_File_Type: GIF
  Data_Set_Credit:
    Source data were acquired during National Oceanic and Atmospheric Administration (NOAA) survey H11250. Please acknowledge NOAA as the originator of the dataset from which this dataset was derived.
  Native_Data_Set_Environment:
    Microsoft Windows XP Version 5.1 (Build 2600) Service Pack 2; ESRI ArcCatalog 9.1.0.780
  Cross_Reference:
    Citation_Information:
      Originator: L.J. Poppe
      Originator: M.L. DiGiacomo-Cohen
      Originator: E.F. Doran
      Originator: S.M. Smith
      Originator: H.F. Stewart
      Originator: N.A. Forfinski
      Publication_Date: 2006
      Title:
        Seafloor character and sedimentary processes in eastern Long Island Sound and Western Block Island Sound
      Series_Information:
        Series_Name: Geo-Marine Letters
        Issue_Identification: v.26, p. 59-68

Data_Quality_Information:
  Attribute_Accuracy:
    Attribute_Accuracy_Report:
      The only attribute value represents hillshaded gridded bathymetry - the grid should be displayed in shades of gray to give impression of a shadded relief map.
  Completeness_Report:
    All collected data were processed and used to generate the gridded data. The area is considered complete; the gaps in the data lie in areas inaccessible to the survey vessels (shallow water surrounding islands).
  Positional_Accuracy:
    Horizontal_Positional_Accuracy:
      Horizontal_Positional_Accuracy_Report:
        Navigation was by differential GPS; positional accuracy to less than 10 m.
  Lineage:
    Source_Information:
      Source_Citation:
        Citation_Information:
          Originator: National Oceanic and Atmospheric Administration
          Publication_Date: Unpublished Material
          Title: B370_03_H11250G_dtm2m_interp.gutm
      Type_of_Source_Media: CD-ROM
      Source_Time_Period_of_Content:
        Time_Period_Information:
          Single_Date/Time:
            Calendar_Date: October 2003
        Source_Currentness_Reference: ground condition
      Source_Citation_Abbreviation: B370_03_H11250G_dtm2m_interp.gutm
      Source_Contribution:
        Digital terrain model with 2 m resolution in .gutm format created by National Oceanic and Atmospheric Administration (NOAA). This data format is used for viewing the model with GeoZui3D software.
    Process_Step:
      Process_Description:
        The multibeam bathymetric data presented herein were collected during October 2003 over a roughly 91 km2 area as part of charting applications aboard the NOAA Survey Vessel Thomas Jefferson. A Simrad EM1002 multibeam system mounted on the hull of this vessel was used to acquire over 560 km of survey lines from the deeper water (>20 m) parts of the study area. Two 29-foot launches with hull-mounted Reson systems were deployed from the ship and were used to acquire an additional 637 km of survey lines from the shallower areas. Horizontal resolution of the data varies with water depth, but averages 2 m. Vertical resolution is about 0.5% of the water depth.
      Source_Used_Citation_Abbreviation: raw data
      Process_Date: 2003
      Source_Produced_Citation_Abbreviation: b370_h11250_dtm2m.gutm
      Process_Contact:
        Contact_Information:
          Contact_Organization_Primary:
            Contact_Organization: National Oceanic and Atmospheric Administration
            Contact_Person: Shep Smith
          Contact_Position: Field Operations Officer
          Contact_Address:
            Address_Type: mailing and physical address
            Address: 439 West York Street
            City: Norfolk
            State_or_Province: VA
            Postal_Code: 23510
            Country: USA
          Contact_Voice_Telephone: (757) 441-6726
          Contact_Electronic_Mail_Address: shep.smith@noaa.gov
    Process_Step:
      Process_Description: The .gutm file was converted to ASCIIgrid format.
      Source_Used_Citation_Abbreviation: b370_h11250_dtm2m.gutm
      Process_Date: 2004
      Source_Produced_Citation_Abbreviation: b370_03.asc
      Process_Contact:
        Contact_Information:
          Contact_Person_Primary:
            Contact_Person: Chris Polloni
            Contact_Organization: U.S. Geological Survey
          Contact_Address:
            Address_Type: mailing and physical address
            Address: 384 Woods Hole Rd
            City: Woods Hole
            State_or_Province: MA
            Postal_Code: 02543-1598
          Contact_Voice_Telephone: (508) 548-8700 x2280
          Contact_Facsimile_Telephone: 508-457-2310
          Contact_Electronic_Mail_Address: cpolloni@usgs.gov
    Process_Step:
      Process_Description:
        The ASCIIgrid was converted to ArcGIS GRID format, and then renamed.
      Source_Used_Citation_Abbreviation: b370_03.asc
      Process_Date: 2004
      Source_Produced_Citation_Abbreviation: B370_03
      Source_Produced_Citation_Abbreviation: h11250u
      Process_Contact:
        Contact_Information:
          Contact_Person_Primary:
            Contact_Person: Mary DiGiacomo-Cohen
            Contact_Organization: U.S. Geological Survey
          Contact_Position: Geologist / GIS Analyst
          Contact_Address:
            Address_Type: mailing and physical address
            Address: Long Island Sound Resource Center
            Address: 1080 Shennecossett Road
            City: Groton
            State_or_Province: CT
            Postal_Code: 06340
          Contact_Voice_Telephone: (860) 405-9210
          Contact_Electronic_Mail_Address: mdicohen@usgs.gov
    Process_Step:
      Process_Description:
        Grid was projected to geographic coordinates using a bilinear interpolation.
      Source_Used_Citation_Abbreviation: h11250u
      Process_Date: 2006
      Source_Produced_Citation_Abbreviation: h11250g
      Process_Contact:
        Contact_Information:
          Contact_Person_Primary:
            Contact_Person: Mary DiGiacomo-Cohen
            Contact_Organization: U.S. Geological Survey
          Contact_Position: Geologist / GIS Analyst
          Contact_Address:
            Address: Long Island Sound Resource Center
            Address: 1080 Shennecossett Road
            City: Groton
            State_or_Province: CT
            Postal_Code: 06340
          Contact_Voice_Telephone: (860) 405-9210
          Contact_Electronic_Mail_Address: mdicohen@usgs.gov
    Process_Step:
      Process_Description:
        Hillshade created with ArcMap. Azimuth of 315, Altitude 30, z factor .000104635 (since cell value or z is in meters, and the x,y coordinates are in decimal degrees, a z factor of .000104635 is approximately equal to a 10 times vertical exaggeration).
      Source_Used_Citation_Abbreviation: h11250g
      Process_Date: 2006
      Source_Produced_Citation_Abbreviation: h11250g_hs
      Process_Contact:
        Contact_Information:
          Contact_Person_Primary:
            Contact_Person: Mary DiGiacomo-Cohen
            Contact_Organization: U.S. Geological Survey
          Contact_Position: Geologist / GIS Analyst
          Contact_Address:
            Address: Long Island Sound Resource Center
            Address: 1080 Shennecossett Road
            City: Groton
            State_or_Province: CT
            Postal_Code: 06340
          Contact_Voice_Telephone: (860) 405-9210
          Contact_Electronic_Mail_Address: mdicohen@usgs.gov
    Process_Step:
      Process_Description:
        The grid was then clipped to remove excess areas of 'no data' surrounding the hillshade grid.
      Source_Used_Citation_Abbreviation: h11250g_hs
      Process_Date: 2006
      Source_Produced_Citation_Abbreviation: h11250g_hs
      Process_Contact:
        Contact_Information:
          Contact_Person_Primary:
            Contact_Person: Mary DiGiacomo-Cohen
            Contact_Organization: U.S. Geological Survey
          Contact_Position: Geologist / GIS Specialist
          Contact_Address:
            Address: Long Island Sound Resource Center
            Address: 1080 Shennecossett Road
            City: Groton
            State_or_Province: CT
            Postal_Code: 06340
          Contact_Voice_Telephone: (860) 405-9210
          Contact_Electronic_Mail_Address: mdicohen@usgs.gov

Spatial_Data_Organization_Information:
  Direct_Spatial_Reference_Method: Raster
  Raster_Object_Information:
    Raster_Object_Type: Grid Cell
    Row_Count: 3966
    Column_Count: 7741
    Vertical_Count: 1

Spatial_Reference_Information:
  Horizontal_Coordinate_System_Definition:
    Geographic:
      Geographic_Coordinate_Units: Decimal degrees
    Planar:
      Planar_Coordinate_Information:
        Planar_Coordinate_Encoding_Method: row and column
        Coordinate_Representation:
          Abscissa_Resolution: 0.000021
          Ordinate_Resolution: 0.000021
    Geodetic_Model:
      Horizontal_Datum_Name: D_WGS_1984
      Ellipsoid_Name: WGS_1984
      Semi-major_Axis: 6378137.000000
      Denominator_of_Flattening_Ratio: 298.257224
  Vertical_Coordinate_System_Definition:
    Depth_System_Definition:

Entity_and_Attribute_Information:
  Detailed_Description:
    Entity_Type:
      Entity_Type_Label: h11250g_hs
    Attribute:
      Attribute_Label: ObjectID
      Attribute_Definition: Internal feature number.
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain:
          Sequential unique whole numbers that are automatically generated.
    Attribute:
      Attribute_Label: Value
    Attribute:
      Attribute_Label: Count
  Overview_Description:

Distribution_Information:
  Distributor:
    Contact_Information:
      Contact_Organization_Primary:
        Contact_Organization: U.S. Geological Survey
        Contact_Person: Larry Poppe
      Contact_Position: Geologist
      Contact_Address:
        Address_Type: mailing and physical address
        Address: 384 Woods Hole Road
        City: Woods Hole
        State_or_Province: MA
        Postal_Code: 02543-1598
        Country: USA
      Contact_Voice_Telephone: 508-548-8700 x2314
      Contact_Facsimile_Telephone: 508-457-2310
      Contact_Electronic_Mail_Address: lpoppe@usgs.gov
  Resource_Description:
    Downloadable Data - H11250G_HS - ArcGIS grid format hillshaded bathymetry image
  Distribution_Liability:
    Although this data set has been used by the U.S. Geological Survey (USGS), National Oceanic and Atmospheric Administration (NOAA), and the Connecticut Department of Environmental Protection (CTDEP), no warranty, expressed or implied, is made by the USGS, NOAA, and the Connecticut DEP as to the accuracy of the data and/or related materials. The act of distribution shall not constitute any such warranty, and no responsibility is assumed by these agencies in the use of these data or related materials.

    Any use of trade, product, or firm names is for descriptive purposes only and does not imply endorsement by the U.S. Government.

  Standard_Order_Process:
    Digital_Form:
      Digital_Transfer_Information:
        Format_Name: ARCG
        Format_Specification: ESRI Raster Grid
        Format_Information_Content:
          One file (h11250g_hs.zip) containing the ArcInfo grid file components, browse graphic, and metadata
        File_Decompression_Technique: zip archive
        Transfer_Size: 22.362
      Digital_Transfer_Option:
        Online_Option:
          Computer_Contact_Information:
            Network_Address:
              Network_Resource_Name:
                <http://pubs.usgs.gov/of/2007/1012/data/bathy/grids/geo/h11250_geo_hlshd2m/h11250g_hs.zip>
              Network_Resource_Name: <http://pubs.usgs.gov/of/2007/1012/html/catalog.html>
          Access_Instructions: Data are downloadable via the World Wide Web (WWW)
        Offline_Option:
          Offline_Media: DVD-ROM
          Recording_Capacity:
            Recording_Density: 4.75
            Recording_Density_Units: Gbytes
          Recording_Format: UDF
    Fees: None
  Technical_Prerequisites:
    The user must have a program similar to ArcGIS that is capable of reading and processing the data files.
  Available_Time_Period:
    Time_Period_Information:
      Single_Date/Time:
        Calendar_Date: 2007

Metadata_Reference_Information:
  Metadata_Date: 20070423
  Metadata_Contact:
    Contact_Information:
      Contact_Organization_Primary:
        Contact_Organization: U.S. Geological Survey
        Contact_Person: Larry Poppe
      Contact_Position: Geologist
      Contact_Address:
        Address_Type: mailing and physical address
        Address: 384 Woods Hole Road
        City: Woods Hole
        State_or_Province: MA
        Postal_Code: 02543-1598
        Country: USA
      Contact_Voice_Telephone: 508-548-8700 x2314
      Contact_Facsimile_Telephone: 508-457-2310
      Contact_Electronic_Mail_Address: lpoppe@usgs.gov
  Metadata_Standard_Name: FGDC Content Standards for Digital Geospatial Metadata
  Metadata_Standard_Version: FGDC-STD-001-1998
  Metadata_Time_Convention: local time
  Metadata_Access_Constraints: None
  Metadata_Use_Constraints: None
  Metadata_Extensions:
    Online_Linkage: <http://www.esri.com/metadata/esriprof80.html>
    Profile_Name: ESRI Metadata Profile

Generated by `mp` version 2.8.6 on Mon Apr 23 09:22:15 2007