### H11250_UTM18_2MMBES.TIF: Color Hill-Shaded GeoTIFF Image Showing the 2-m bathymetry Generated from NOAA Survey H11250 in Eastern Long Island Sound (UTM Zone 18)

Metadata also available as Outline | Text

#### Frequently-anticipated questions:

- What does this data set describe?
  1. How should this data set be cited?
  2. What geographic area does the data set cover?
  3. What does it look like?
  4. Does the data set describe conditions during a particular time period?
  5. What is the general form of this data set?
  6. How does the data set represent geographic features?
  7. How does the data set describe geographic features?
- Who produced the data set?
  1. Who are the originators of the data set?
  2. Who also contributed to the data set?
  3. To whom should users address questions about the data?
- Why was the data set created?
- How was the data set created?
  1. From what previous works were the data drawn?
  2. How were the data generated, processed, and modified?
  3. What similar or related data should the user be aware of?
- How reliable are the data; what problems remain in the data set?
  1. How well have the observations been checked?
  2. How accurate are the geographic locations?
  3. How accurate are the heights or depths?
  4. Where are the gaps in the data? What is missing?
  5. How consistent are the relationships among the data, including topology?
- How can someone get a copy of the data set?
  1. Are there legal restrictions on access or use of the data?
  2. Who distributes the data?
  3. What's the catalog number I need to order this data set?
  4. What legal disclaimers am I supposed to read?
  5. How can I download or order the data?
- Who wrote the metadata?

### What does this data set describe?

Title:
  H11250_UTM18_2MMBES.TIF: Color Hill-Shaded GeoTIFF Image Showing the 2-m bathymetry Generated from NOAA Survey H11250 in Eastern Long Island Sound (UTM Zone 18)
Abstract:
  The U.S. Geological Survey, in cooperation with the National Oceanic and Atmospheric Administration and the Connecticut Department of Environmental Protection, has produced detailed geologic maps of the sea floor in Long Island Sound, a major East Coast estuary surrounded by the most densely populated region of the United States. These studies have built upon cooperative research with the State of Connecticut that was initiated in 1982. The current phase of this research program is directed toward studies of sea-floor sediment distribution, processes that control sediment distribution, nearshore environmental concerns, and the relation of benthic community structures to the sea-floor geology.

  Anthropogenic wastes, toxic chemicals, and changes in land-use patterns resulting from residential, commercial, and recreational development have stressed the environment of the Sound, causing degradation and potential loss of benthic habitats (Koppelman and others, 1976; Long Island Sound Study, 1994). Detailed maps of the sea floor are needed to help evaluate the extent of adverse impacts and to help manage resources wisely in the future. Therefore, in a continuing effort to better understand Long Island Sound, we have constructed and interpreted mulitbeam bathymetric data within specific areas of special interest. The color GeoTIFF of hill-shaded bathymetry in UTM Zone 18 projection presented herein covers a roughly 94 km square area of the sea floor in the area known as the Race at the eastern end of Long Island Sound. The original multibeam bathymetric data were collected during October 2003 as part of charting applications aboard the NOAA Survey Vessel Thomas Jefferson. A Simrad EM1002 multibeam system mounted on the hull of this vessel was used to acquire over 560 km of survey lines from the deeper water (>20 m) parts of the study area. Two 29-foot launches with hull-mounted Reson systems were deployed from the ship and were used to acquire an additional 637 km of survey lines from the shallower areas.

  Detailed bathymetic data and their interpretations serve many purposes, including: (1) defining the geological variability of the sea floor, which is one of the primary controls of benthic habitat diversity; (2) improving our understanding of the processes that control the distribution and transport of bottom sediments and the distribution of benthic habitats and associated infaunal community structures; and (3) providing a detailed framework for future research, monitoring, and management activities. The bathymetric data models also serve as base maps for subsequent sedimentological, geochemical, and biological observations, because precise information on environmental setting is important for selection of sampling sites and for accurate interpretation of point measurements.

1. How should this data set be cited?

   > U.S. Geological Survey, 2007, H11250_UTM18_2MMBES.TIF: Color Hill-Shaded GeoTIFF Image Showing the 2-m bathymetry Generated from NOAA Survey H11250 in Eastern Long Island Sound (UTM Zone 18): Open-File Report 2007-1012, U.S. Geological Survey, Coastal and Marine Geology Program, Woods Hole Science Center, Woods Hole, MA.

   > Online Links:

   > - <http://pubs.usgs.gov/of/2007/1012/data/bathy/geotifs/utm/h11250_utm18_2mmbes.zip>
   > - <http://pubs.usgs.gov/of/2007/1012/data/bathy/geotifs/utm/>
   > - <http://pubs.usgs.gov/of/2007/1012/html/catalog.html>

   This is part of the following larger work.

   > Poppe, L.J., DiGiacomo-Cohen, M.L., Doran, E.F., Smith, S.M., Stewart, H.F., and Forfinski, N.A., 2007, Geologic Interpretation and Multibeam Bathymetry of the Sea Floor in the Vicinity of the Race, Eastern Long Island Sound: Open-File Report 2007-1012, U.S. Geological Survey, Coastal and Marine Geology Program, Woods Hole Science Center, Woods Hole, MA.

   > Online Links:

   > - <http://pubs.usgs.gov/of/2007/1012/>

   Other_Citation_Details: 1 DVD-ROM

2. What geographic area does the data set cover?

   West_Bounding_Coordinate: -72.154000
   East_Bounding_Coordinate: -71.992004
   North_Bounding_Coordinate: 41.270997
   South_Bounding_Coordinate: 41.188000

3. What does it look like?

   <http://pubs.usgs.gov/of/2007/1012/data/bathy/geotifs/utm/h11250_utm18_2mmbes.gif> (GIF)
     Thumbnail image showing the color hill-shaded GeoTIFF of the 2-m bathymetry from NOAA survey H11250 in UTM, Zone 18.

4. Does the data set describe conditions during a particular time period?

   Calendar_Date: 2003
   Currentness_Reference: ground condition

5. What is the general form of this data set?

   Geospatial_Data_Presentation_Form: remote-sensing image

6. How does the data set represent geographic features?

   1. How are geographic features stored in the data set?

      This is a Raster data set. It contains the following raster data types:

      - Dimensions 4069 x 6141 x 1, type Pixel

   2. What coordinate system is used to represent geographic features?

      Grid_Coordinate_System_Name: Universal Transverse Mercator
      Universal_Transverse_Mercator:
        UTM_Zone_Number: 18
        Transverse_Mercator:
          Scale_Factor_at_Central_Meridian: .999600
          Longitude_of_Central_Meridian: -75.000000
          Latitude_of_Projection_Origin: 0.000000
          False_Easting: 500000.000000
          False_Northing: 0.000000

      Planar coordinates are encoded using row and column
      Abscissae (x-coordinates) are specified to the nearest 2.317044
      Ordinates (y-coordinates) are specified to the nearest 2.317144
      Planar coordinates are specified in meters

      The horizontal datum used is North American Datum of 1983.
      The ellipsoid used is WGS84.
      The semi-major axis of the ellipsoid used is 6378137.000000.
      The flattening of the ellipsoid used is 1/298.257224.

      Vertical_Coordinate_System_Definition:
        Depth_System_Definition:

7. How does the data set describe geographic features?

### Who produced the data set?

1. Who are the originators of the data set? (may include formal authors, digital compilers, and editors)

   - U.S. Geological Survey

2. Who also contributed to the data set?

   > Source data were acquired during National Oceanic and Atmospheric Administration (NOAA) survey H11250. Please acknowledge NOAA as the originator of the dataset from which this dataset was derived.

3. To whom should users address questions about the data?

   Larry Poppe
   U.S. Geological Survey
   Geologist
   384 Woods Hole Road
   Woods Hole, MA 02543-1598
   USA

   508-548-8700 x2314 (voice)
   508-457-2310 (FAX)
   lpoppe@usgs.gov

### Why was the data set created?

> To release a color GeoTIFF image of the 2-m bathymetry generated from NOAA survey H11250 in easternmost Long Island Sound and westernmost Block Island Sound. This hill-shaded GeoTIFF in UTM Zone 18 serves as a starting point for a geologic study of the area surrounding the Race in eastern Long Island Sound and can be used as a base for interpretative layers. The GeoTIFF can be used in ArcMap or ArcView to dramatically display the varied bathymetry and geologic features of the area.

### How was the data set created?

1. From what previous works were the data drawn?

   (source 1 of 1)
     Type_of_Source_Media: DVD-ROM
     Source_Contribution:
       The original multibeam bathymetric data acquired with Simrad EM1002, Reson 8101, and 8125 echosounder systems during NOAA cruise H11250 aboard the NOAA ship Thomas Jefferson.

2. How were the data generated, processed, and modified?

   (process 1 of 4)
     The multibeam bathymetric data presented herein were collected during October 2003 over a roughly 91 km2 area as part of charting applications aboard the NOAA Survey Vessel Thomas Jefferson. A Simrad EM1002 multibeam system mounted on the hull of this vessel was used to acquire over 560 km of survey lines from the deeper water (>20 m) parts of the study area. Two 29-foot launches with hull-mounted Reson systems were deployed from the ship and were used to acquire an additional 637 km of survey lines from the shallower areas. Horizontal resolution of the data varies with water depth, but averages 2 m. Vertical resolution is about 0.5% of the water depth.

     Person who carried out this activity:

     Shep Smith
     National Oceanic and Atmospheric Admnistration
     Field Operations Officer
     439 West York Street
     Norfolk, VA 23510
     USA

     757-441-6726 (voice)
     shep.smith@noaa.gov

     Contact_Instructions:
     Data sources used in this process:
     - raw bathymetric data

     Data sources produced in this process:

     - b370_h11250_dtm2m.gutm

   Date: 2004 (process 2 of 4)
     The .gutm file was converted to ASCIIgrid format.

     Person who carried out this activity:

     Chris Polloni
     U.S. Geological Survey
     384 Woods Hole Road
     Woods Hole, MA 02543

     508-548-8700 x2280 (voice)
     508-457-2310 (FAX)
     cpolloni@usgs.gov

     Data sources used in this process:
     - b370_h11250_dtm2m.gutm

     Data sources produced in this process:

     - b370_03.asc

   Date: 2004 (process 3 of 4)
     The ASCIIgrid was converted to ArcGIS GRID format, and then renamed.

     Person who carried out this activity:

     Mary DiGiacomo-Cohen
     U.S. Geological Survey
     Geologist/GIS Analyst
     Long Island Sound Resource Center
     Groton, CT 06340
     USA

     860-405-9210 (voice)
     mdicohen@usgs.gov

     Data sources used in this process:
     - b370_03.asc

     Data sources produced in this process:

     - H11250U

   Date: 2006 (process 4 of 4)
     The grid was hill-shaded (sun-illuminated) with the sun at an azimuth of 315, an altitude angle above the horizon of 30, a verticle exaggeration of ~10x (z factor .000104635), a 40 % transparency overlying the grid displayed with a continous color pallete and no linear stretch, and exported as a GeoTIFF image.

     Person who carried out this activity:

     Mary DiGiacomo-Cohen
     U.S. Geological Survey
     Geologist/GIS Analyst
     Long Island Sound Resource Center
     Groton, CT 06340

     860-405-9210 (voice)
     mdicohen@usgs.gov

     Data sources used in this process:
     - H11250U

     Data sources produced in this process:

     - h11250_utm18_2mmbes.tif

3. What similar or related data should the user be aware of?

   > Poppe, L.J., DiGiacomo-Cohen, M.L., Smith, S.M., Stewart, H.F., and Forfinski, N.A., 2006, Seafloor character and sedimentary processes in eastern Long Island Sound and Western Block Island Sound: Geo-Marine Letters v. 26, p. 59-68.

### How reliable are the data; what problems remain in the data set?

1. How well have the observations been checked?

2. How accurate are the geographic locations?

   Navigation was by differential GPS

3. How accurate are the heights or depths?

4. Where are the gaps in the data? What is missing?

   All collected data were processed and used to produce this dataset. The area is considered complete; the gaps in the data lie in areas inaccessible to the survey vessels (shallow water surrounding islands).

5. How consistent are the relationships among the observations, including topology?

### How can someone get a copy of the data set?

> Are there legal restrictions on access or use of the data?

> > Access_Constraints: None
> > Use_Constraints:
> >   Public domain data are freely redistributable with proper metadata and source attribution. Please recognize the U.S. Geological Survey (USGS) and the Connecticut Department of Environmental Protection (CTDEP) as the originators of this data set.

1. Who distributes the data set? (Distributor 1 of 1)

   U.S. Geological Survey
   c/o Larry Poppe
   Geologist
   384 Woods Hole Road
   Woods Hole, MA 02543-1598

   508-548-8700 x2314 (voice)
   508-457-2310 (FAX)
   lpoppe@usgs.gov

2. What's the catalog number I need to order this data set?

   `Downloadable Data`

3. What legal disclaimers am I supposed to read?

   > Although this data set has been used by the U.S. Geological Survey (USGS), National Oceanic and Atmospheric Administration (NOAA), and the Connecticut Department of Environmental Protection (CTDEP), no warranty, expressed or implied, is made by the USGS, NOAA, and the Connecticut DEP as to the accuracy of the data and/or related materials. The act of distribution shall not constitute any such warranty, and no responsibility is assumed by these agencies in the use of these data or related materials.

   > Any use of trade, product, or firm names is for descriptive purposes only and does not imply endorsement by the U.S. Government.

4. How can I download or order the data?

   - Availability in digital form:

     Data format: | A zip archive containing the GeoTIFF image, associated world file, browse graphic and metadata. in format TIFF GeoTIFF Size: 0.000
     Network links: | <http://pubs.usgs.gov/of/2007/1012/data/bathy/geotifs/utm/h11250_utm18_2mmbes.zip> <http://pubs.usgs.gov/of/2007/1012/data/bathy/geotifs/utm/> <http://pubs.usgs.gov/of/2007/1012/html/catalog.html>
     Media you can order: | DVD-ROM (Density 4.75 Gbytes) (format UDF)

   - Cost to order the data: None

5. What hardware or software do I need in order to use the data set?

   > This image is available as a GeoTIFF image with an accompanying world file. To utilize this data, the user must have an image viewer, image processing or GIS software package capable of importing a GeoTIFF image.

### Who wrote the metadata?

Dates:
  Last modified: 06-Apr-2007
Metadata author:
  U.S. Geological Survey
  c/o Larry Poppe
  Geologist
  384 Woods Hole Road
  Woods Hole, MA 02543-1598
  USA

  508-548-8700 x2314 (voice)
  508-457-2310 (FAX)
  lpoppe@usgs.gov

Metadata standard:
  FGDC Content Standards for Digital Geospatial Metadata (FGDC-STD-001-1998)
Metadata extensions used:
  - <http://www.esri.com/metadata/esriprof80.html>

Generated by `mp` version 2.8.6 on Fri Apr 06 09:26:04 2007